{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":59,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DB-O"]
[]
[]
[]
[]
["","","","","","BDB710DB13XXA","BDB710DB13XXB","MDB106EA12XXA","MDB106EA12XXB","MDB107EA12XXA","MDB107EA12XXB","BDB110DA12XXA","BDB110DA12XXB","BDB112DA12XXA","BDB112DA12XXB","BDB117DA12XXA","BDB117DA12XXB","BDB713DB13XXA","BDB713DB13XXB","MDB212EB12XXA","MDB212EB12XXB","BDB218DA12XXA","BDB218DA12XXB","BDB220DB12XXA","BDB220DB12XXB","PDB221TO02DA","PDB221TO02DB","MDB315EB13XXA","MDB315EB13XXB","BDB320DB13XXA","BDB320DB13XXB","MDB320EB13XXA","MDB320EB13XXB","BDB330DB13XXA","BDB330DB13XXB","PDB330DB11XXA","PDB330DB11XXB","MDB425EB13XXA","MDB425EB13XXB","BDB440DB13XXA","BDB440DB13XXB","BDB445DB13XXA","BDB445DB13XXB","MDB530EB13XXA","MDB530EB13XXB","BDB550DB13XXA","BDB550DB13XXB","MDB635EB13XXA","MDB635EB13XXB","MDB645EB13XXA","MDB645EB13XXB","BDB660DB13XXA","BDB660DB13XXB","BDB680DB13XXA","BDB680DB13XXB","MDB706EB13XXA","MDB706EB13XXB","MDB707EB13XXA","MDB707EB13XXB"]
["Refrigerating capacity","Low temperature","R-452A","Nom","kW","11.537","","","","","","0.662","","0.905","","1.164","","12.735","","","","1.436","","1.719","","","","","","2.384","","","","2.581","","","","","","3.283","","3.604","","","","4.925","","","","","","7.492","","8.94"]
["","Medium temperature","R-134a","Nom","kW","","","1.14","","1.422","","","","","","","","","","1.816","","","","","","","","3.188","","","","3.492","","","","","","3.948","","","","","","5.07","","","","7.293","","8.779","","","","","","11.014","","14.069"]
["Casing","Colour","","Condensing unit","","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White"]
["Dimensions","Condensing unit","","Width","mm","1725","","682","","682","","682","","682","","682","","1725","","882","","882","","882","","882","","882","","882","","882","","882","","882","","920","","920","","920","","1075","","1075","","1575","","1575","","1575","","1575","","1725","","1725"]
["","","","Depth","mm","770","","337","","337","","337","","337","","337","","770","","427","","427","","427","","427","","427","","427","","427","","427","","427","","540","","540","","540","","560","","560","","670","","670","","670","","670","","770","","770"]
["","Evaporator unit","","Height","mm","","544","","215","","215","","215","","215","","215","","544","","215","","215","","215","","215","","215","","215","","215","","215","","215","","545","","545","","545","","544","","544","","544","","544","","544","","544","","544","","544"]
["","","","Width","mm","","1975","","676","","676","","676","","676","","676","","1975","","1074","","1074","","1074","","1074","","1676","","1676","","1676","","1676","","1676","","845","","845","","845","","1425","","1425","","1975","","1975","","1975","","1975","","1975","","1975"]
["","","","Depth","mm","","608","","410","","410","","410","","410","","410","","608","","410","","410","","410","","410","","410","","410","","410","","410","","410","","690","","690","","690","","608","","608","","608","","608","","608","","608","","608","","608"]
["Compressor","Quantity","","","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1"]
["","Type","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic"]
["","Model","","","","S 10-52Y","","NJ6220Z","","NTU6222ZV","","NEU2178GK","","NJ2192GK","","NJ2212GK","","S 15-56Y","","TFH4518Y/T","","NJ2212GK","","TFH2480Z/T","","TFH2480Z/T","","TFH4525Y/T","","TFH2511Z/T","","MTZ40JH4VE","","NTZ068A4","","NTZ068A4","","MTZ50HK4CVE","","NTZ096A4LR1B","","NTZ108A4LR1B","","MTZ64HM4","","NTZ 136A4LR1B","","MTZ80HP4","","MTZ100HS4","","NTZ215A4LR1B","","NTZ271A4 LR1B","","MTZ125HU4","","MTZ160HW4VE"]
["","Starting method","","","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct"]
["Condenser","Air flow","","","m³/h","8100","","750","","750","","750","","750","","750","","8100","","1400","","1400","","1400","","1400","","1500","","1500","","1500","","1500","","1500","","3150","","3150","","3150","","3200","","3200","","5500","","7000","","7000","","7000","","8100","","8100"]
["Defrost","","","","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric"]
["Defrost heaters","W","","","","6400","","450","","450","","450","","450","","450","","6400","","800","","800","","800","","800","","1400","","1400","","1400","","1400","","1400","","1400","","1400","","1400","","3150","","3250","","4900","","4900","","5000","","5000","","6300","","6300"]
["Evaporator","Air throw","","","m","","18","","4","","4","","4","","4","","4","","18","","4","","4","","4","","4","","4","","4","","4","","4","","4","","12","","12","","12","","17","","17","","20","","20","","20","","20","","18","","18"]
["Operation range","Cold room temperature","","Min.","°C","-25","","-5","","-5","","-25","","-25","","-25","","-25","","-5","","-25","","-25","","-5","","-5","","-25","","-5","","-25","","-5","","-5","","-25","","-25","","-5","","-25","","-5","","-5","","-25","","-25","","-5","","-5"]
["","","","Max.","°C","-15","","10","","10","","-15","","-15","","-15","","-15","","10","","-15","","-15","","10","","10","","-15","","10","","-15","","10","","10","","-15","","-15","","10","","-15","","10","","10","","-15","","-15","","10","","10"]
["","Ambient temperature","","Min.","°C","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20"]
["","","","Max.","°C","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45"]
["Refrigerant","Type","","","","R-452A","","R-134a","","R-134a","","R-452A","","R-452A","","R-452A","","R-452A","","R-134a","","R-452A","","R-452A","","R-452A","","R-134a","","R-452A","","R-134a","","R-452A","","R-452A","","R-134a","","R-452A","","R-452A","","R-134a","","R-452A","","R-134a","","R-134a","","R-452A","","R-452A","","R-134a","","R-134a"]
["","GWP","","","","2140","","1430","","1430","","2140","","2140","","2140","","2140","","1430","","2140","","2140","","2140","","1430","","2140","","1430","","2140","","2140","","1430","","2140","","2140","","1430","","2140","","1430","","1430","","2140","","2140","","1430","","1430"]
["Standard liquid receiver","l","","","","15","","1.6","","2.5","","1.6","","1.6","","1.6","","15","","2.5","","2.5","","2.5","","2.5","","2.5","","2.5","","2.5","","2.5","","2.5","","5.6","","5.6","","5.6","","10","","10","","15","","15","","15","","15","","15","","15"]
["Power supply","Voltage","","","V","380-400","","220-230","","220-230","","220-230","","220-230","","220-230","","380-400","","380-400","","220-230","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400"]
["","Phase","","","","3N~","","1~","","1~","","1~","","1~","","1~","","3N~","","3N~","","1~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~"]
["","Frequency","","","Hz","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50"]