{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-B"]
[]
[]
[]
[]
["","","","","FTXC20BV1B","FTXC25BV1B","FTXC35BV1B","FTXC50BV1B","FTXC60BV1B","FTXC71BV1B"]
["Sound pressure level","Cooling","Medium","dBA","33","33","34","39","42","42"]
["","","Silent operation","dBA","20","20","21","29","30","30"]
["","","Low","dBA","26","26","26","33","38","38"]
["","","High","dBA","38","38","39","45","46","46"]
["Control systems","Infrared remote control","","","BRC52B66","BRC52B66","BRC52B66","BRC52B66","BRC52B66","BRC52B66"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Drain","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Power input","Cooling","Nom.","kW","0.595","0.765","1.045","1.55","1.89","2.38"]
["","Heating","Nom.","kW","0.67","0.75","1.07","1.515","1.68","2.46"]
["Sound power level","Cooling","","dBA","54","54","55","57","60","60"]
["Dimensions","Unit","Width","mm","785","785","785","785","1,005","1,005"]
["","","Depth","mm","250","250","250","250","288","288"]
["","","Height","mm","288","288","288","288","297","297"]
["Casing","Material","","","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene"]
["","Colour","","","White","White","White","White","White","White"]
["Weight","Unit","","kg","9.0","9.0","9.5","9.5","13.0","13.0"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240","220-240"]