{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N9"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B9","RXTP35N2V1B9"]
["Sound pressure level","Heating","","Nom.","dBA","49","49"]
["","Cooling","","Nom.","dBA","48","48"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Charge","","","kg","1.1","1.1"]
["","Type","","","","R-32","R-32"]
["Fan motor","Speed","Cooling","Super low","rpm","450","450"]
["","","Heating","Super low","rpm","360","360"]
["Operation range","Cooling","Ambient","Max.","°CDB","46","46"]
["","","","Min.","°CDB","-10","-10"]
["","Heating","Ambient","Max.","°CWB","18","18"]
["","","","Min.","°CWB","-25","-25"]
["Piping connections","Level difference","IU - OU","Max.","m","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","763","763"]
["","","","Depth","mm","312","312"]
["","","","Height","mm","551","551"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","38","38"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range"]
["","","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]